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Air filters and dust collectors
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Survey Form #1 for Selecting Air Purification Filters in Ventilation Systems.
	№
	Questions
	Entry field

	1
	Purpose of the room into which purified air will be supplied.
	

	
	
	

	2
	Type or cleanliness class of the room.
	

	3
	For clean rooms - maximum permissible number of particles of maximum size per cubic meter of purified air, pcs/m³.
	

	4
	Concentration of dust and other potential impurities in the air at the inlet of the filter, mg/m³.
	

	5
	Requirements for the concentration of dust in the purified air, mg/m³.
	

	6
	Maximum permissible particle size in purified air, µm.
	

	7
	Need for gas pollutant removal.
	

	8
	Filter class according to GOST R 51251-99 (EN 779; EN 1822).
	

	9
	Volume flow rate of the purified air, m³/h.
	

	10
	Maximum allowable filter resistance (pressure drop), Pa.
	

	11
	Requirements for the dimensional parameters for filter placement (length, height, depth), mm.
	

	12
	Required data for replacing existing cell (cassette) filters: panel, pocket (bag), and pleated filters.

Dimensional parameters of the inlet section, mm.
	

	
	- Height
	

	
	- Width
	

	
	- Depth (in the direction of airflow)
	

	
	- Length of pockets (for pocket filters)
	

	
	- Number of pockets (for pocket filters), pcs.
	

	
	- Housing material
	

	13
	Continuous operation requirement for filters, hours.
	

	14
	Organization Name

Mailing Address

Contact Person (Full Name, Position)

Phone, Fax, E-mail

Date Compiled
	

	
	
	

	
	
	

	
	
	

	
	
	


We kindly request that you return the completed survey form to us by a convenient method for you: fax, e-mail, or postal mail.
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