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Air filters and dust collectors
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Survey Form #2 for Selecting Dust Collection Equipment in Exhaust Ventilation Systems.
	№
	Questions
	Entry field

	1
	Type of production, brief description of the manufacturing process.
	

	
	
	

	
	
	

	2
	Volume flow rate of cleaned gases (air), m³/h.
	

	3
	Temperature of cleaned gases, °C.
	

	4
	Humidity of cleaned gases, %, dew point, °C.
	

	5
	Operating time and frequency of operation of the technological equipment, hours/day.
	

	6
	Possible fluctuations in air flow rate (min, max), m³/h.
	

	7
	Dust concentration at the inlet, g/m³.
	

	8
	Approximate particle size distribution of dust, micrometers/fractions, %.
	

	
	Up to 2 μm
	2-5 μm
	5-10 μm
	10-20 μm
	20-40 μm
	40-100 μm
	More than 100 μm

	%
	
	
	
	
	
	
	

	9
	Types of dust, % content by types.
	

	
	
	

	10
	Dust properties (abrasiveness, corrosiveness, moisture content, angle of repose, cohesion, flowability, combustibility, explosiveness).
	

	11
	Dust density, g/cm³ (kg/m³)
	

	12
	Bulk density of dust, kg/m³.
	

	13
	Required dust concentration in the air after purification, mg/m³.
	

	14
	Requirement for the recirculation of purified air.
	

	15
	Range of outdoor temperatures, °C.
	

	16
	Required pressure (vacuum) in the dust collector housing, Pa.
	

	17
	Dimensions of the platform (other dimensional requirements for filter placement).
	

	
	
	

	18
	Ability to place the dust collector in a heated room.
	

	19
	Required elevation level for dust discharge flanges from hoppers, meters.
	

	20
	Availability of compressed air, pressure, quality of purification, and drying.
	

	21
	Availability of technical water.
	

	22
	Presence of purification facilities.
	

	23
	Special requirements for automation.
	

	24
	Special requirements.
	

	25
	Organization Name

Mailing Address

Contact Person (Full Name, Position)

Phone, Fax, E-mail

Date Compiled
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