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Air filters and dust collectors
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Survey Form #4 
for Selecting Cartridge Filter Elements of the FEP Type
	№
	Questions
	Entry field

	1
	Type of production, brief description of the manufacturing process.
	

	
	
	

	2
	Volume flow rate of cleaned gases (air), nm³/h
	

	3
	Temperature of cleaned gases, ºC
	

	4
	Humidity of cleaned gases, %
	

	5
	Dust properties (abrasiveness, corrosiveness, moisture content, angle of repose, cohesion, flowability, combustibility, explosiveness)
	

	Structural features of FEP (cartridge filter elements)

	6
	Diameter (outer (D), inner (d)), mm

For conical FEPs, it is necessary to specify 4 diameters
	

	7
	Recommended diameters D/d, mm
	Выберите из предлагаемого ряда или напишите свои размеры

	
	155/69; 200/90; 220/142; 234/125; 325/195; 325/215; 325/225; 360/250; 420/290; 520/380; 560/400
	

	8
	Length, mm
	

	9
	Presence of internal mesh yes/no
	

	10
	Presence of external mesh yes/no
	

	11
	Number of external clamps
	

	12
	Direction of air inlet: outside/inside
	

	13
	Sketches of end caps (top and bottom) must be attached to the survey form (hand-drawn is acceptable).
	

	14 

	1 - Support mesh;

2 - Metal end cap;

3 - Mini-pleated filter cartridge;

4 - Clamping belt;

5 - End ring;

6 - Rubber seal.
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Figure: Schematic diagram of the cartridge filter element (FEP).

	15
	Organization Name

Mailing Address

Contact Person (Full Name, Position)

Phone, Fax, E-mail

Date Compiled
	


Please return the completed survey form to us using a convenient method for you: fax, email, or postal mail.
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